{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"merged":[[0,0,0,5],[12,0,12,5]],"flags":["formulas_cached_only"]}
["2022年电力工程学院内涵建设内容更新采购项目清单"]
["项目","参数及尺寸","单位","数量","单价（元）","金额（元）"]
["发光字暗藏背架","主体材质： 25mm方通1.0厚304不锈钢暗藏背架\n工    艺： 激光切割、无缝激光焊接、精工打磨，抛光、电镀、喷汽车漆等；\n颜 色 节：银灰不锈钢原色（按样板订购）   \n底板厚度：18mm\n尺    寸:   2X3mm\n安    装：  焊接、打钉、支撑、防水密、结构胶等；","个",6]
["门口发光字（里建校区电力工程学院）","主体材质： 1.2mm厚304不锈钢、底部结皮PVC、亚克力密封，内涵LED灯（国际蓝景牌）、内发光 、密封防水；\n工    艺： 激光切割、无缝激光焊接、精工打磨，抛光、电镀、喷汽车漆（红色）等；\n字    体：隶书\n颜 色 节：古铜不锈钢（按样板订购）\n色    温: 6000K（可调）\n厚    度: 80mm(选项)   \n底板厚度：18mm\n尺    寸: 2mX2m\n安    装：  焊接、打钉、支撑、防水密、结构胶等；\n★含门口北京澄通LED屏幕P10模块维修及200W 5V40A电源更换，为保证LED屏幕维修更换质量须提供LED屏原厂型号配件及供货方售后承诺书。","平米",24]
["6楼发光字（里建校区电力工程学院）","主体材质： 1.2mm厚304不锈钢、底部结皮PVC、面克力密封，内涵LED灯（国际蓝景牌）、内发光 、密封防水；\n工    艺： 激光切割、无缝激光焊接、精工打磨，抛光、电镀、喷汽车漆等；\n字    体：隶书\n颜 色 节：红色不锈钢（按样板订购）\n色    温: 6000K（可调）\n厚    度: 80mm(选项)   \n底板厚度：18mm\n尺    寸:   0.95mX1.2m\n安    装：  焊接、打钉、支撑、防水密，\n包含6楼布线到1楼：4平方铜心线、20mmPVC线管，安装：卡扣、拼接、楼层开孔等；\n★含门口学校石头重新描红（汽车漆），静湖石重新描字，确保3年不褪色。","平米",25.08]
["户内宣传栏制作","60*80厘米，主材：5mm+5mm透明亚克力（伸美牌），户外写真、广告钉等：\n工艺：切割、打磨、抛光、开孔\n安装：水平、打孔、打胶粒、螺丝固定","块",36]
["外墙翻新","1、墙面基层处理。\n2、破裂和开裂等情况，用腻子粉进行修复。\n3、先刷专业底漆一道。\n4、再刷面漆2道。\n5、分色纸打磨的砂纸等辅材和人工。","平米",100]
["门口右侧不锈钢宣传栏","采用：25mm1.0mm厚304不锈钢方通，60mm圆管1.0mm厚304不锈钢，4mm铝塑板，挖坑、混凝土、切割焊接，1.2米乘2.4米，栏顶做美化防雨设计，户外彩色车贴制作内容，含安装。","平米",11.52]
["宣传栏内容更新","需要更改的所有宣传栏，户外写真，含安装","平米",57.6]
["电力大家庭文化墙更换内容","主材：20mm结皮PVC内容UV，过水晶膜\n安装：拆、装、含设计","平米",28]
["软膜灯箱置换内容","软膜,0.9米乘1.2米，含更换安装","张",20]
[{"$nulls":4},"合计（元):"]
["以上价格含税，包括运输、安装、调试等工程费用"]
["报价单位（公司名称）：",null,null,"联系人：",null,"联系电话："]