{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["竞赛用耗材、工具"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"竞赛用耗材、工具","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"merged":[[0,0,0,7],[35,1,35,2]],"flags":["formulas_cached_only"]}
["2020年智能供配电系统安装与调试学生技能竞赛耗材采购清单"]
["序号","名称","规格","单位","数量","单价(元)","小计（元）","备注"]
[1,"电线（黑色）","BVR1.0（国标）","卷",200,null,null,"每卷100米长，按1个队比赛（培训、练习）1次用2卷（200米）计"]
[2,"电线(黑色)","BLV10（国标）","卷",8,null,null,"每卷100米长，按1个队比赛（培训、练习）1次用10米计"]
[3,"电缆","RVV4*2.5+1","米",200]
[4,"插针","E1008","包",10,null,null,"一包为1000个"]
[5,"接线端子","UT1.5-5","包",10,null,null,"一包为1000个"]
[6,"接线端子","UT1.5-3","包",10,null,null,"一包为1000个"]
[7,"接线端子","OT1.5-10","包",3,null,null,"一包为1000个"]
[8,"接线端子","OT10-12","包",1,null,null,"一包为500个"]
[9,"接线端子","SC10-8","包",2,null,null,"一包为500个"]
[10,"按压式快速接线端子","SPL-2","个",10]
[11,"按压式快速接线端子","SPL-3","个",10]
[12,"色管（黄绿红）","10平方线","套",30,null,null,"黄绿红各1个为1套,一个队一次用4套"]
[13,"塑料自封袋","透明自封拉链袋，材质: PE塑料，厚度双层12丝，尺寸：30*40cm及以上规格，每包数量不少于50只","包",1,null,null,"装耗材，一个队用一个袋子"]
[14,"选手竞赛马甲","通用码","套",40]
[15,"双锁盖元件分类收纳箱","茶花牌，透明收纳箱，容量：58L及以上，透明顶盖，双锁盖扣","个",10,null,null,"装耗材，一个队用一个"]
[16,"线号管","1平方线","套",100,null,null,"号码100—150为1套，一个队一次用4套"]
[17,"尼龙扎带（黑色）","3*150cm（黑色）","包",80,null,null,"一个队比赛（培训和练习）用1次1包"]
[18,"缠绕管","直径6mm","包",80,null,null,"一个队比赛（培训和练习）用1次1包"]
[19,"熔断器","RT28-32X/4A","个",60,null,null,"比赛过程中应急更换"]
[20,"熔断器","RT28-32X/6A","个",70,null,null,"比赛过程中应急更换"]
[21,"免焊对接端子","2EDGRK3.81-3P直针","对",80,null,null,"比赛过程中应急更换"]
[22,"免焊对接端子","2EDGRK3.81-4P直针","对",80,null,null,"比赛过程中应急更换"]
[23,"免焊对接端子","2EDGRK3.81-10P直针","对",80,null,null,"比赛过程中应急更换"]
[24,"端子排","UK-2.5B   800V  32A","个",700,null,null,"比赛过程中应急更换"]
[25,"万用表","数字式 VICTOR 88B","个",6]
[26,"电动操作机构","LCD2","个",16,null,null,"比赛过程中应急更换"]
[27,"按钮(红，绿)","AD26B-22DS","对",20,null,null,"比赛过程中应急更换"]
[28,"万能转换开关","LW12-16","个",20,null,null,"比赛过程中应急更换"]
[29,"智能单相电流表","DEA194I-9K1-R  AC 5A 等级0.5 \n电源AC/DC36V 面板96*96","个",6,null,null,"比赛过程中应急更换"]
[30,"智能三相电流表","DED194E-9S4-R  AC400V 5A 等级0.5 \n电源AC/DC36V  面板96*96","个",4,null,null,"比赛过程中应急更换"]
[31,"键盘","USB接口  87键","个",5,null,null,"比赛过程中应急更换"]
[32,"鼠标","USB接口  1500dpi以上","个",5,null,null,"比赛过程中应急更换"]
[33,"工具套装（包含工具箱）","至少包含：\n1、针型端子压线钳，材质:镍铬合金钢，1把\n2、叉型端子压线钳，材质:镍铬合金钢，1把\n3、小一字和十字螺丝刀，2.4*40mm，各1把\n4、长柄螺丝刀十字，PH1*150mm，1把\n5、剥线钳，0.2-1.2m㎡，1把\n6、内六角扳手，9件套，1套\n7、绝缘手套，10kV，1双\n8、尖嘴钳，1把\n9、塑料工具箱，16寸，1个。","套",20]
[null,"合计"]