{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"merged":[[0,0,0,7],[6,1,6,4],[7,1,7,7],[8,1,8,7],[9,1,9,7]],"flags":["formulas_cached_only"]}
["机电工程学院外墙门头招牌发光字内涵更换内容制作清单"]
["序号","项目","参数","数量","单位","单价","金额","备注"]
[1,"拆除原有字","切割分解、处理等",1,"项"]
[2,"机电工程学院（门头招牌）","\n主体材质：1.2厚304不锈钢、底部10mm结皮PVC、内置LED灯带（蓝景牌）\n工艺：隐藏背架、激光切割，激光无缝焊接、精工打磨，抛光、电镀、喷汽车漆、螺丝固定、防水密封等。\n颜色调节：灰色汽车漆打底、红色\n厚度：80mm\n字体：方正大黑体\n底板厚度：10mm\n色温：6000K\n尺寸：2mX2m\n安装：撬开隔热板安装、焊接、打钉、支撑、防水密封等。\n\n★为了质量保障本项乙方要提供样板、产品合格证、及检测报告，盖章文件，不提供报价无效。\n\n",24,"平方"]
[3,"钢结构、隐藏背架、混凝土上支撑点","主体材质：40mmX40mm1.0厚不锈钢方通背架\n工艺：隐藏背架、切割、焊接精工打磨、抛光、\n打混凝土隔热层立点结构抓地固定等。\n厚度：40mm\n尺寸：2mX3m\n安装：焊接、打钉、支撑、防水密封、暗藏布线等。\n★为了质量保障本项乙方要提供样板、产品合格证、及检测报告，盖章文件，不提供报价无效。",30,"平方"]
[4,"拉电布线","输入主线4平方铜芯线、2.5平方铜芯线输出、线管、天维管、波纹管、胶布、电箱、时控开关（可根据昼夜自动开关）等。",1,"项"]
[12,{"$nulls":4},"合计："]
[13,"注：以上制作含安装、运费及发票税金。"]
{"$rows_empty":14}
[null,"报价公司（公司名称）：",null,null,"联系人：",null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}